{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["About","fitting","Line Sizing (Single Phase)"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":3,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"About","index":0,"n_rows":1,"n_cols":4,"rows_kept":1,"cut":false,"hidden":false,"merged":[[0,3,43,11]]}
[null,null,null,"Line Sizing\n\nBY  EIEPD"]

{"sheet":"fitting","index":1,"n_rows":50,"n_cols":34,"rows_kept":50,"cut":false,"hidden":false,"merged":[[4,1,4,33],[10,1,10,33],[45,1,45,21],[38,1,38,27]]}
[]
[]
[null,0]
[]
[null,"    PIPE CHARACHTERISTICS (STANDARD PIPE)"]
[null,"Internal Area","mm2",{"$f":"3.14159*D7^2/4","v":196.03685075777236},{"$f":"3.14159*E7^2/4","v":344.04192672767351},{"$f":"3.14159*F7^2/4","v":557.58094573749088},1313.4353471563097,2164.9003020471878,2164.9003020471878,4769.4429501530867,8213.050418195342,12906.947907392874,18638.826176748895,32275.395248111046,50873.590613260436,72965.815358399981,88958.756658743718,117841.05857144372,150777.01689294374,187766.63162324374,228809.90276234373,273906.83031024371,323057.41426694364,376261.65463244368,433519.55140674365,494831.10458984372,560196.31418174366,629615.18018244358,703087.70259194379,780613.88141024357,862193.71663734375,947827.20827324351,1037514.3563179437,1131255.1607714435]
[null,"Internal Diameter ","mm",{"$f":"D8*25.4","v":15.798799999999998},{"$f":"E8*25.4","v":20.929599999999997},{"$f":"F8*25.4","v":26.644599999999997},40.893999999999998,52.501800000000003,52.501800000000003,77.927199999999999,102.26039999999999,128.19379999999998,154.05099999999999,202.7174,254.50799999999998,304.79999999999995,336.54999999999995,387.34999999999997,438.15,488.95,539.75,590.54999999999995,641.34999999999991,692.15,742.94999999999993,793.75,844.55,895.34999999999991,946.15,996.94999999999993,1047.75,1098.55,{"$f":"AG8*25.4","v":1149.3499999999999},{"$f":"AH8*25.4","v":1200.1499999999999}]
[null,"Internal Diameter","in",0.622,0.82399999999999995,1.0489999999999999,1.61,2.0670000000000002,2.0670000000000002,3.0680000000000001,4.0259999999999998,5.0469999999999997,6.0650000000000004,7.9809999999999999,10.02,12,13.25,15.25,17.25,19.25,21.25,23.25,25.25,27.25,29.25,31.25,33.25,35.25,37.25,39.25,41.25,43.25,45.25,47.25]
[null,"Friction factor (FT)",null,2.7E-2,2.5000000000000001E-2,2.3E-2,2.1000000000000001E-2,1.9E-2,1.7999999999999999E-2,1.7999999999999999E-2,1.7000000000000001E-2,1.6E-2,1.4999999999999999E-2,1.4E-2,1.4E-2,1.2999999999999999E-2,1.2999999999999999E-2,1.2999999999999999E-2,1.2E-2,1.2E-2,1.2E-2,1.2E-2,1.0999999999999999E-2,1.0999999999999999E-2,1.0999999999999999E-2,1.0999999999999999E-2,1.0999999999999999E-2,0.01,0.01,0.01,0.01,0.01,0.01,0.01]
[null,"Nominal Pipe Size","in",0.5,0.75,1,1.5,2,2.5,3,4,5,6,8,10,12,14,16,18,20,22,24,26,28,30,32,34,36,38,40,42,44,46,48]
[null,"fittings K value extracted from Crane"]
[null,"  * tee flow thru","20*ft",{"$f":"20*D9","v":0.54},{"$f":"20*E9","v":0.5},0.45999999999999996,0.42000000000000004,0.38,0.36,0.36,0.34,0.32,0.3,0.28000000000000003,0.28000000000000003,0.26,0.26,0.26,0.24,0.24,0.24,0.24,0.21999999999999997,0.21999999999999997,0.21999999999999997,0.21999999999999997,0.21999999999999997,0.2,0.2,0.2,0.2,0.2,0.2,0.2]
[null,"  * tee branch","60*ft",{"$f":"60*D9","v":1.6199999999999999},{"$f":"60*E9","v":1.5},1.38,1.26,1.1399999999999999,1.0799999999999998,1.0799999999999998,1.02,0.96,0.89999999999999991,0.84,0.84,0.77999999999999992,0.77999999999999992,0.77999999999999992,0.72,0.72,0.72,0.72,0.65999999999999992,0.65999999999999992,0.65999999999999992,0.65999999999999992,0.65999999999999992,0.6,0.6,0.6,0.6,0.6,0.6,0.6]
[null,"  * elbow 90 deg LR ","14*ft",{"$f":"14*D9","v":0.378},{"$f":"14*E9","v":0.35000000000000003},0.32200000000000001,0.29400000000000004,0.26600000000000001,0.252,0.252,0.23800000000000002,0.224,0.21,0.19600000000000001,0.19600000000000001,0.182,0.182,0.182,0.16800000000000001,0.16800000000000001,0.16800000000000001,0.16800000000000001,0.154,0.154,0.154,0.154,0.154,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,"  * elbow 90 deg screwed","30*ft",{"$f":"30*D9","v":0.80999999999999994},{"$f":"30*E9","v":0.75},0.69,0.63,0.56999999999999995,0.53999999999999992,0.53999999999999992,0.51,0.48,0.44999999999999996,0.42,0.42,0.38999999999999996,0.38999999999999996,0.38999999999999996,0.36,0.36,0.36,0.36,0.32999999999999996,0.32999999999999996,0.32999999999999996,0.32999999999999996,0.32999999999999996,0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,"  * elbow 45 deg","16*ft",{"$f":"16*D9","v":0.432},{"$f":"16*E9","v":0.4},0.36799999999999999,0.33600000000000002,0.30399999999999999,0.28799999999999998,0.28799999999999998,0.27200000000000002,0.25600000000000001,0.24,0.224,0.224,0.20799999999999999,0.20799999999999999,0.20799999999999999,0.192,0.192,0.192,0.192,0.17599999999999999,0.17599999999999999,0.17599999999999999,0.17599999999999999,0.17599999999999999,0.16,0.16,0.16,0.16,0.16,0.16,0.16]
[null,"  * elbow 45 deg screwed","16*ft",{"$f":"16*D9","v":0.432},{"$f":"16*E9","v":0.4},0.36799999999999999,0.33600000000000002,0.30399999999999999,0.28799999999999998,0.28799999999999998,0.27200000000000002,0.25600000000000001,0.24,0.224,0.224,0.20799999999999999,0.20799999999999999,0.20799999999999999,0.192,0.192,0.192,0.192,0.17599999999999999,0.17599999999999999,0.17599999999999999,0.17599999999999999,0.17599999999999999,0.16,0.16,0.16,0.16,0.16,0.16,0.16]
[null,"  * gate valve","8*ft",{"$f":"8*D9","v":0.216},{"$f":"8*E9","v":0.2},0.184,0.16800000000000001,0.152,0.14399999999999999,0.14399999999999999,0.13600000000000001,0.128,0.12,0.112,0.112,0.104,0.104,0.104,9.6000000000000002E-2,9.6000000000000002E-2,9.6000000000000002E-2,9.6000000000000002E-2,8.7999999999999995E-2,8.7999999999999995E-2,8.7999999999999995E-2,8.7999999999999995E-2,8.7999999999999995E-2,0.08,0.08,0.08,0.08,0.08,0.08,0.08]
[null,"  * ball valve","3*ft",{"$f":"3*D9","v":8.1000000000000003E-2},{"$f":"3*E9","v":7.5000000000000011E-2},6.9000000000000006E-2,6.3E-2,5.6999999999999995E-2,5.3999999999999992E-2,5.3999999999999992E-2,5.1000000000000004E-2,4.8000000000000001E-2,4.4999999999999998E-2,4.2000000000000003E-2,4.2000000000000003E-2,3.9E-2,3.9E-2,3.9E-2,3.6000000000000004E-2,3.6000000000000004E-2,3.6000000000000004E-2,3.6000000000000004E-2,3.3000000000000002E-2,3.3000000000000002E-2,3.3000000000000002E-2,3.3000000000000002E-2,3.3000000000000002E-2,0.03,0.03,0.03,0.03,0.03,0.03,0.03]
[null,"  * globe  valve","340*ft",{"$f":"340*D9","v":9.18},{"$f":"340*E9","v":8.5},7.82,7.1400000000000006,6.46,6.1199999999999992,6.1199999999999992,5.78,5.44,5.0999999999999996,4.76,4.76,4.42,4.42,4.42,4.08,4.08,4.08,4.08,3.7399999999999998,3.7399999999999998,3.7399999999999998,3.7399999999999998,3.7399999999999998,3.4,3.4,3.4,3.4,3.4,3.4,3.4]
[null,"  * butterfly valve","45*ft /35/25 ***",{"$f":"45*D9","v":1.2150000000000001},{"$f":"45*E9","v":1.125},1.0349999999999999,0.94500000000000006,0.85499999999999998,0.80999999999999994,0.80999999999999994,0.76500000000000001,0.72,0.67499999999999993,0.63,0.63,0.58499999999999996,0.58499999999999996,0.58499999999999996,0.54,0.54,0.54,0.54,0.495,0.495,0.495,0.495,0.495,0.45,0.45,0.45,0.45,0.45,0.45,0.45]
[null,"  * check valve swing","50*ft",{"$f":"50*D9","v":1.35},{"$f":"50*E9","v":1.25},1.1499999999999999,1.05,0.95,0.89999999999999991,0.89999999999999991,0.85000000000000009,0.8,0.75,0.70000000000000007,0.70000000000000007,0.65,0.65,0.65,0.6,0.6,0.6,0.6,0.54999999999999993,0.54999999999999993,0.54999999999999993,0.54999999999999993,0.54999999999999993,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[null,"  * check valve lift","600*ft",{"$f":"600*D9","v":16.2},{"$f":"600*E9","v":15},13.799999999999999,12.600000000000001,11.4,10.799999999999999,10.799999999999999,10.200000000000001,9.6,9,8.4,8.4,7.8,7.8,7.8,7.2,7.2,7.2,7.2,6.6,6.6,6.6,6.6,6.6,6,6,6,6,6,6,6]
[null,"  * check valvestop lift","400*ft",{"$f":"400*D9","v":10.8},{"$f":"400*E9","v":10},9.1999999999999993,8.4,7.6,7.1999999999999993,7.1999999999999993,6.8000000000000007,6.4,6,5.6000000000000005,5.6000000000000005,5.2,5.2,5.2,4.8,4.8,4.8,4.8,4.3999999999999995,4.3999999999999995,4.3999999999999995,4.3999999999999995,4.3999999999999995,4,4,4,4,4,4,4]
[null,"  * check valve tilting disk","40*ft******",{"$f":"40*D9","v":1.08},{"$f":"40*E9","v":1},0.91999999999999993,0.84000000000000008,0.76,0.72,0.72,0.68,0.64,0.6,0.56000000000000005,0.56000000000000005,0.52,0.52,0.52,0.48,0.48,0.48,0.48,0.43999999999999995,0.43999999999999995,0.43999999999999995,0.43999999999999995,0.43999999999999995,0.4,0.4,0.4,0.4,0.4,0.4,0.4]
[null,"  * foot valve hinged disc","75*ft",{"$f":"75*D9","v":2.0249999999999999},{"$f":"75*E9","v":1.875},1.7249999999999999,1.5750000000000002,1.425,1.3499999999999999,1.3499999999999999,1.2750000000000001,1.2,1.125,1.05,1.05,0.97499999999999998,0.97499999999999998,0.97499999999999998,0.9,0.9,0.9,0.9,0.82499999999999996,0.82499999999999996,0.82499999999999996,0.82499999999999996,0.82499999999999996,0.75,0.75,0.75,0.75,0.75,0.75,0.75]
[null,"  * foot valve poppet disc","420*ft",{"$f":"420*D9","v":11.34},{"$f":"420*E9","v":10.5},9.66,8.82,7.9799999999999995,7.56,7.56,7.1400000000000006,6.72,6.3,5.88,5.88,5.46,5.46,5.46,5.04,5.04,5.04,5.04,4.62,4.62,4.62,4.62,4.62,4.2,4.2,4.2,4.2,4.2,4.2,4.2]
[null,"  * reducer N*K"," ",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"  * entrance"," ",0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78,0.78]
[null,"  * exit",null,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[]
[]
[]
[null,{"$f":"CELL(\"FILENAME\")","v":"C:\\Users\\Behrouzi\\Downloads\\[EIEPD Line Sizing (1).xlsm]Line Sizing (Single Phase)"}]
[]
[]
[]
[null," "]
[null,"SCHEDULE 40"]
[null,"Nominal Pipe Size","in",0.5,0.75,1,1.5,2,2.5,3,4,5,6,8,10,12,14,16,18,20,22,24,26,28,30,32,34,36]
[null,"INTERNAL DIAMETER   ","in",0.622,0.82399999999999995,1.0489999999999999,1.61,2.0670000000000002,2.0670000000000002,3.0680000000000001,4.0259999999999998,5.0469999999999997,6.0650000000000004,7.9809999999999999,10.02,11.938000000000001,13.124000000000001,15,16.876000000000001,18.812000000000001,null,22.623999999999999,null,null,null,30.623999999999999,32.624000000000002,34.5]
[null,"INTERNAL DIAMETER  ","mm",{"$f":"D41*25.4","v":15.798799999999998},20.929599999999997,26.644599999999997,40.893999999999998,52.501800000000003,52.501800000000003,77.927199999999999,102.26039999999999,128.19379999999998,154.05099999999999,202.7174,254.50799999999998,{"$f":"P41*25.4","v":303.22519999999997},333.34960000000001,381,428.65039999999999,477.82479999999998,null,574.64959999999996,null,null,null,777.8495999999999,828.64959999999996,876.3]
[null,"INTERNAL AREA     ","mm2",{"$f":"3.14159*D42^2/4","v":196.03685075777236},344.04192672767351,557.58094573749088,1313.4353471563097,2164.9003020471878,2164.9003020471878,4769.4429501530867,8213.050418195342,12906.947907392874,18638.826176748895,32275.395248111046,50873.590613260436,{"$f":"3.14159*P42^2/4","v":72213.783048267607},87274.906296264118,114009.0864975,144309.8519680801,179319.23932805567,null,259355.66109213067,null,null,null,475204.757547913,539301.17268385866,603108.06757177494]
[]
[]
[null,"SCHEDULE 80"]
[null,"Nominal Pipe Size","in",0.5,0.75,1,1.5,2,2.5,3,4,5,6,8,10,12,14,16,18,20,22,24]
[null,"INTERNAL DIAMETER   ","in",0.54600000000000004,0.74199999999999999,0.95699999999999996,1.278,1.9390000000000001,2.323,2.9,3.8260000000000001,4.8129999999999997,5.7610000000000001,7.625,9.5619999999999994,11.374000000000001,12.5,14.311999999999999,16.123999999999999,17.937999999999999,19.75,21.562000000000001]
[null,"INTERNAL DIAMETER  ","mm",{"$f":"D48*25.4","v":13.868399999999999},{"$f":"E48*25.4","v":18.846799999999998},24.307799999999997,32.461199999999998,49.250599999999999,59.004199999999997,73.66,97.180399999999992,122.25019999999999,146.32939999999999,193.67499999999998,242.87479999999996,288.89960000000002,317.5,363.52479999999997,409.54959999999994,455.62519999999995,501.65,547.6748]
[null,"INTERNAL AREA     ","mm2",{"$f":"3.14159*D49^2/4","v":151.05747924572759},{"$f":"3.14159*E49^2/4","v":278.97466088182034},464.06714604288379,827.59651924881234,1905.0771408687428,2734.3579543554115,4261.4062997509991,7417.3176651479025,11737.853130812913,16817.16163051108,29460.26464286093,46329.160049875209,65551.614955030469,79172.976734374999,103790.49970519185,131735.40978798247,163044.06220024917,197647.41911969372,235578.16315111204]

{"sheet":"Line Sizing (Single Phase)","index":2,"n_rows":37,"n_cols":54,"rows_kept":37,"cut":false,"hidden":false,"merged":[[32,4,32,5],[36,1,42,7],[34,1,34,2],[35,1,35,2],[34,4,34,7],[35,4,35,7],[32,1,32,2],[6,1,6,7],[10,1,10,2],[10,3,10,5],[10,6,10,7],[12,1,12,2],[12,4,12,5],[13,1,13,2],[11,6,13,7],[14,6,14,7],[15,6,15,7],[18,1,18,3],[18,4,18,5],[15,4,15,5],[11,1,11,2],[11,4,11,5],[13,4,13,5],[14,1,14,2],[14,4,14,5],[15,1,15,2],[19,1,19,2],[19,4,19,5],[20,1,20,2],[20,4,20,5],[23,1,23,2],[23,4,23,5],[22,1,22,2],[22,4,22,5],[25,1,25,2],[25,4,25,5],[28,1,28,2],[28,4,28,5],[26,4,26,5],[27,4,27,5],[1,2,1,4],[2,2,2,4],[3,2,3,4],[4,2,4,4],[0,9,32,9],[21,1,21,2],[21,4,21,5],[1,5,4,5],[31,1,31,2],[31,4,31,5],[29,1,29,2],[29,4,29,5],[30,1,30,2],[30,4,30,5],[24,1,24,2],[24,4,24,5]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CS",1.8E-3,null,"STD",null,"Vapor",null,{"$f":"IF(E13=AZ1,\"ρV²\",\"Velocity\")","v":"ρV²"}]
[null,"PROJECT : ","Methanol Plant",null,null,null,"DATE :","2023.02.01",null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CCS",1.7999999999999999E-2,null,"40",null,"Liquid"]
[null,"SUBJECT :","EIEPD",null,null,null,"BY  :","EIEPD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SS / SL",1.1999999999999999E-3,null,"80"]
[null,"REF FILE : ","Line Sizing Calculation,sheet2",null,null,null,"REV  :",3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SS / WLD",2.8999999999999998E-3]
[null,"UNIT  :",null,null,null,null,"DOC NO.:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Titanium / SL",1.1999999999999999E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Titanium / WLD",2.8999999999999998E-3]
[null,"Line Sizing Calculation Form (Single Phase)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Galvanid CS",5.8999999999999999E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GRP",8.0000000000000004E-4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELP",5.8999999999999999E-3]
[]
[null,"Line No. :",null,3315,null,null,"Service (From/To)"]
[null,"Total Flow Rate",null,"kg/hr",1578,null,"Recycle H2"]
[null,"Fluid phase (Liquid/Vapor)",null," ","Vapor"]
[null,"Temperature",null,"C",48]
[null,"Density",null,"kg/m3",25,null,"Material"]
[null,"Viscosity",null,"Cp",1.4999999999999999E-2,null,"CS"]
[]
[]
[null,"Calculation Results ",null,null,"Trial 1",null,"Trial 2","Trial 3"]
[null,"Pipe Length          (DEF.)",null,"m",1000,null,1000,1000]
[null,"Nominal Pipe Size",null,"inch",3,null,4,6]
[null,"Schedule No.",null,null,"80",null,"80","40"]
[null,"Line Roughness    (DEF.)",null,"inch",{"$f":"VLOOKUP($G$16,$AU$1:$AV$9,2,0)","v":1.8E-3},null,{"$f":"VLOOKUP($G$16,$AU$1:$AV$9,2,0)","v":1.8E-3},{"$f":"VLOOKUP($G$16,$AU$1:$AV$9,2,0)","v":1.8E-3}]
[null,"Pipe Internal Diameter",null,"mm",{"$f":"IF(E22=\"STD\",OFFSET(fitting!$B$7,0,find_col(E21)-2,1,1),IF(E22=\"40\",OFFSET(fitting!B42,0,find_col(E21)-2,1,1),IF(E22=\"80\",OFFSET(fitting!B49,0,find_col(E21)-2,1,1),\"Range Out\")))","v":73.66},null,{"$f":"IF(G22=\"STD\",OFFSET(fitting!$B$7,0,find_col(G21)-2,1,1),IF(G22=\"40\",OFFSET(fitting!B42,0,find_col(G21)-2,1,1),IF(G22=\"80\",OFFSET(fitting!B49,0,find_col(G21)-2,1,1),\"Range Out\")))","v":97.180399999999992},{"$f":"IF(H22=\"STD\",OFFSET(fitting!$B$7,0,find_col(H21)-2,1,1),IF(H22=\"40\",OFFSET(fitting!B42,0,find_col(H21)-2,1,1),IF(H22=\"80\",OFFSET(fitting!B49,0,find_col(H21)-2,1,1),\"Range Out\")))","v":154.05099999999999}]
[null,"Pipe Internal Area",null,"mm2",{"$f":"3.14159*E24^2/4","v":4261.4062997509991},null,{"$f":"3.14159*G24^2/4","v":7417.3176651479025},{"$f":"3.14159*H24^2/4","v":18638.826176748895}]
[null,"Reynold 's No.",null," ",{"$f":"IF(L2=1,353.658*E12/E16/E24,353.658*E12/2.2046/E16/E24)","v":505088.53651914204},null,{"$f":"IF(L2=1,353.658*E12/E16/G24,353.658*E12/2.2046/E16/G24)","v":382842.85308560164},{"$f":"IF(L2=1,353.658*E12/$E$16/H24,353.658*E12/2.2046/$E$16/H24)","v":241509.7701410572}]
[null,"Y",null,null,{"$f":"(-2.457 *0.3678*LOG((7 / E26) ^ 0.9 + 0.27 * E23 *25.4/ E24,2.71828)) ^ 16","v":138382080917691.72},null,{"$f":"(-2.457 *0.3678 *LOG((7 / G26) ^ 0.9 + 0.27 * G23 *25.4/G24,2.71828)) ^ 16","v":181944136512611.59},{"$f":"(-2.457 *0.3678* LOG((7 / H26) ^ 0.9 + 0.27 * H23 *25.4/ H24,2.71828)) ^ 16","v":222953162725148.59}]
[null,"Z",null,null,{"$f":"(37530 /E26) ^ 16","v":8.6333001574315365E-19},null,{"$f":"(37530 /G26) ^ 16","v":7.2732468098867688E-17},{"$f":"(37530 /H26) ^ 16","v":1.1563831566877283E-13}]
[null,"Friction Factor",null,null,{"$f":"((8 / E26) ^ 12 + 1 / (E27 + E28) ^ 1.48) ^ (1/12)","v":1.8027416153157713E-2},null,{"$f":"((8 / G26) ^ 12 + 1 / (G27 + G28) ^ 1.48) ^ (1 / 12)","v":1.7429073662529083E-2},{"$f":"((8 / H26) ^ 12 + 1 / (H27 + H28) ^ 1.48) ^ (1 / 12)","v":1.69975757273725E-2}]
[null,"Head Loss (Dh/L)",null,"bar",{"$f":"51.02*E29*E31^2/E24","v":0.21138069222381417},null,{"$f":"51.02*G29*G31*G31/G24","v":5.1129470825596296E-2},{"$f":"51.02*H29*H31*H31/H24","v":4.9814385770302382E-3}]
[null,"Velocity",null,"m/s",{"$f":"IF(L2=1,E12*1000000/3600/E25/E15,E12*1000000/2.2/3600/E25/(E15*1000/62.4)/0.3048)","v":4.1144476963761552},null,{"$f":"IF(L2=1,E12*1000000/3600/G25/E15,E12*1000000/3600/2.2/G25/(E15*1000/62.4)/0.3048)","v":2.3638374578074264},{"$f":"IF(L2=1,E12*1000000/3600/H25/E15,E12*1000000/3600/2.2/H25/(E15*1000/62.4)/0.3048)","v":0.94068870899206003}]
[null,"Pressure Drop (DP) ",null,"bar",{"$f":"IF(L2=1,500*E31^2*E15*E29*E20/E24/101300,500*(E31*0.3048)^2*(E15*1000/62.4)*E29*(E20/0.3048)/E24/101300)","v":0.51124070981545611},null,{"$f":"IF(L2=1,500*G31^2*E15*G29*G20/G24/101300,500*(G31*0.3048)^2*(E15*1000/62.4)*G29*(G20/0.3048)/G24/101300)","v":0.12366061763904862},{"$f":"IF(L2=1,500*H29*H20*H31^2*E15/H24/101300,500*(H31*0.3048)^2*(H20/0.3048)*H29*(E15*1000/62.4)/H24/101300)","v":1.2047998174433651E-2}]
[null,"ρV²",null,"kg/m.s2",{"$f":"$E$15*E31*E31","v":423.21699615537625},null,{"$f":"$E$15*G31*G31","v":139.69318817333689},{"$f":"$E$15*H31*H31","v":22.122381180628715}]
[]
[null,{"$f":"\"Allowable \"&BB1","v":"Allowable ρV²"},null,{"$f":"IF(E13=AZ1,IF(D15=\"kg/m3\",\"kg/m.s2\",\"Ib/ft.s2\"),IF(D15=\"kg/m3\",\"m/s\",\"ft/s\"))","v":"kg/m.s2"},7500]
[null,"Allowable Pressure Drop",null,"bar/1000m","****"]
[null,"NOTES:\n       \n\n"]