{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["T-5004","Calculate"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"T-5004","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[[3,1,3,3],[3,5,3,7],[0,1,1,7],[19,1,20,7],[21,1,21,7]]}
[null,"Calculation of TowerSizing"]
[]
[]
[null,"Inlet Stream",null,null,null,"Outlet Stream"]
[null,"Parameter","Value","Unit",null,"Parameter","Value","Unit"]
[null,"L",8197,"kg/h",null,"L",8524,"kg/h"]
[null,"G",11332,"kg/h",null,"G",11004,"kg/h"]
[null,"Lm",{"$f":"C6/3600","v":2.2769444444444447},"kg/s",null,"Lm",{"$f":"G6/3600","v":2.367777777777778},"kg/s"]
[null,"Gm",{"$f":"C7/3600","v":3.1477777777777778},"kg/s",null,"Gm",{"$f":"G7/3600","v":3.0566666666666666},"kg/s"]
[null,"ρl",989,null,null,"ρl",964]
[null,"ρv",1.1499999999999999,null,null,"ρv",1.1100000000000001]
[null,"F",{"$f":"(C8/C9)*((C11/C10)^0.5)","v":2.4666023652662687E-2},null,null,"F",{"$f":"(G8/G9)*((G11/G10)^0.5)","v":2.6285475138305248E-2}]
[]
[null,"C",0.03,null,null,"C",1.7500000000000002E-2]
[null,"Fp",18,null,null,"Fp",18]
[null,"G^2",{"$f":"(2.99*C11*(C10-C11)*C14)/(((0.567)^0.1)*((1000/C10)^0.1)*C15)","v":5.9850820112248631},null,null,"G^2",{"$f":"(2.99*G11*(G10-G11)*G14)/(((0.567)^0.1)*((1000/G10)^0.1)*G15)","v":3.2763160141824152}]
[null,"G",{"$f":"C16^0.5","v":2.4464427259236752},null,null,"G",{"$f":"G16^0.5","v":1.8100596714424679}]
[null,"D",{"$f":"(C9/(C17*0.7854))^0.5","v":1.2799383673245897},null,null,"D",{"$f":"(G9/(G17*0.7854))^0.5","v":1.4663314378490524}]
[]
[null,"By M.Behrouzi   Educational Institute of Equipment and Process Design"]
[]
[null,"https://www.linkedin.com/in/mohammadrezabehrouzi"]

{"sheet":"Calculate","index":1,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[[3,1,3,3],[3,5,3,7],[0,1,1,7],[19,1,20,7],[21,1,21,7]]}
[null,"Calculation of TowerSizing"]
[]
[]
[null,"Inlet Stream",null,null,null,"Outlet Stream"]
[null,"Parameter","Value","Unit",null,"Parameter","Value","Unit"]
[null,"L",null,"kg/h",null,"L",null,"kg/h"]
[null,"G",null,"kg/h",null,"G",null,"kg/h"]
[null,"Lm",{"$f":"C6/3600","v":0},"kg/s",null,"Lm",{"$f":"IFERROR(G6/3600,\"\")","v":0},"kg/s"]
[null,"Gm",{"$f":"C7/3600","v":0},"kg/s",null,"Gm",{"$f":"IFERROR(G7/3600,\"\")","v":0},"kg/s"]
[null,"ρl",null,null,null,"ρl"]
[null,"ρv",null,null,null,"ρv"]
[null,"F",{"$f":"IFERROR((C8/C9)*((C11/C10)^0.5),\"\")","v":""},null,null,"F",{"$f":"IFERROR((G8/G9)*((G11/G10)^0.5),\"\")","v":""}]
[]
[null,"C",null,null,null,"C"]
[null,"Fp",null,null,null,"Fp"]
[null,"G^2",{"$f":"IFERROR((2.99*C11*(C10-C11)*C14)/(((0.567)^0.1)*((1000/C10)^0.1)*C15),\"\")","v":""},null,null,"G^2",{"$f":"IFERROR((2.99*G11*(G10-G11)*G14)/(((0.567)^0.1)*((1000/G10)^0.1)*G15),\"\")","v":""}]
[null,"G",{"$f":"IFERROR(C16^0.5,\"\")","v":""},null,null,"G",{"$f":"IFERROR(G16^0.5,\"\")","v":""}]
[null,"D",{"$f":"IFERROR((C9/(C17*0.7854))^0.5,\"\")","v":""},null,null,"D",{"$f":"IFERROR((G9/(G17*0.7854))^0.5,\"\")","v":""}]
[]
[null,"By M.Behrouzi   Educational Institute of Equipment and Process Design"]
[]
[null,"https://www.linkedin.com/in/mohammadrezabehrouzi"]